**application of the cableway then adapter forest wheeled tractors**

Michaela Hnilicová1, Valéria Messingerová2, Miroslav Dado3, Pavel Beňo1

*1Institution, Department, Faculty, University, Address, Postcode, City, State, e-mail*

*2Institution, Department, Faculty, University, Address, Postcode, City, State, e-mail*

*3Institution, Department, Faculty, University, Address, Postcode, City, State, e-mail*

**Abstract:** Field conditions, high proportion of mountain forests and forest health condition requires ecological forest machinery. Skidding by cable systems is the most ecologically friendly skidding method. On the basis of the need of greater use of timber skidding by cable systems we started to work on a proposal of cable system based on transportation-circulating cable as adapters of forest wheeled tractors.

**Key words:** skidding, cable system, forest wheeled tractors, adapters

**Introduction**

The extended abstract briefly summarizes the main procedures and results of the paper. It should not exceed the range of 2 pages. The introduction should be brief and factual. It must contain the formulation of a scientific problem and the relationship of the solved work to previous works with similar issues. Finally, the scope and objectives of the contribution need to be clearly defined.

**material and methods**

Contains a brief description of materials, methods, and procedures. The main goal of this section is to provide enough detail for a competent researcher.

**results**

In this part it is necessary to focus on the evaluation of the achieved results. Provide figures, tables, and equations if necessary.

Fig. 1Database file of grinders divided by correlation between weight and power

Obr. 1 Databázový súbor drvičov rozdelený podľa závislosti hmotnosti od výkonu

Table 1 The categorization of forestry mulchers

Tabuľka 1 Kategorizácia drvičov

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **K1t** | **K2t** | **K3t** | **K4t** | **K5t** | **K6t** |
| Engine performance[kW] | 0 ÷ 75 | 75 ÷ 100 | 100 ÷ 125 | 125 ÷ 175 | 175 ÷ 225 | < 225 |
| Weight  [t] | 0 ÷ 1,3 | 1,3 ÷ 1,7 | 1,7 ÷ 2,0 | 2,0 ÷ 2,8 | 2,8 ÷ 3,5 | < 3,5 |
| Grinding diameter [cm] | 0 ÷ 22 | 22 ÷ 26 | 26 ÷ 30 | 30 ÷ 38 | 38 ÷ 46 | < 46 |
|  | **K1hm** | **K2hm** | **K3hm** | **K4hm** | **K5hm** | **K6hm** |
| Flow rating  [kW] | 0 ÷ 75 | 75 ÷ 100 | 100 ÷ 150 | 150 ÷ 175 | 175 ÷ 200 | < 200 |
| Weight  [t] | 0 ÷ 0,55 | 0,55 ÷ 0,7 | 0,7 ÷ 1,0 | 1,0 ÷ 1,2 | 1,2 ÷ 1,35 | < 1,35 |
| Grinding diameter [cm] | 0 ÷ 12 | 12 ÷ 16 | 16 ÷ 23 | 23 ÷ 26 | 26 ÷ 30 | < 30 |

Equations should be formatted as follows:

(1)

where *ηG* is flow hydraulic pump efficiency [-],

*Q* is flow rate [m3.s-1],

*VG* is geometric volume of hydrogenerator [m3.ot-1].

**conclusion**

It should present a summary of the major results of the work and deduct fulfillment of set goals.

*Contribution has been prepared within the solving of scientific grant project VEGA-0145-10 "Development of adapters for mechanization of work on the creation and raising of the forest."*

**literature**

List only the literature used in the extended abstract.

AAPB, The association for applied psychophysiology and biofeedback http://www.aapb.org/i4a/pages/index.cfm?pageid=3336 [accessed September 2013].

DADO, M., HNILICA, R., 2009. Control Measures for Minimizing exposure to Metal Working Fluid Aerosols. *J. Saf. Res. Appl*. (3) [online]. ISSN 1803-3687. Available in: <http://www.bozpinfo.cz/josra/josra-03-2009/dado\_hnilicaaerosoly.html>.

DADO, M., SCHWARZ, M., HNILICA, R., 2013. Metalworking Fluid Mist Characterization for the Turning Process: a Preliminary Study. In: Hudec, J. (ed.): *7th Annual International Conference 2013: Manufacturing Systems Today and Tomorrow*. Technical University of Liberec, 2013.

www page of LKT s.r.o., Trstená. [online] [cit. 2014-01-27]. Available on: <http://www.lkttrstena.sk/fotogaleria/brezovica-2010>.

GELLERSTEDT, S., 2002. Operation of the Single-Grip Harvester: Motor-Sensory and Cognitive Work. *International Journal of Forest Engineering* 13(2), pp 35-47. DOI:10.1080/14942119.2002.10702461.

LEHRER, P., SMETANKIN, A., POTAPOVA, T., 2000. Respiratory sinus arrhythmia biofeedback therapy for asthma a report of 20 unmedicated pediatric cases using the Smetaniknnnn method. *Applied psychophysiology and biofeedback* 25(3). Netherlands: Springer; 2000. pp. 193–200. ISSN 1573-3270.

NESTORIUC, Y., MARTIN, A., RIEF, W., ANDRASIK, F., 2008. Biofeedback treatment for headache disorders a comprehensive efficacy review applied psychophysiology and biofeedback. *Appl Psychophysiol Biofeedback* (2008) 33:125–140 DOI 10.1007/s10484-008-9060-3.

PURFÜRST, F. T., 2010. Learning Curves of Harvester Operators. *Croatian Journal of Forest Engineering* 31(2), pp 89-97. ISSN 1845-5719

STANOVSKÝ, M., FERENČÍK, M., SLUGEŇ, J., 2006. Evaluation of certain performance parameters of LKT 82 C. In: Hudec, J. (ed.): *Trends in forestry, wood and environmental technology and its application in the manufacturing process. International scientific conference on 10. anniversary of FEVT Zvolen.* Technical university in Zvolen, Zvolen, 2006, s. 190 – 197, ISBN 80-228-1648-5.

**Corresponding author:**

Name Surname, tel., e-mail: